## Keyboard shortcuts

Press `←` or `→` to navigate between chapters

Press `S` or `/` to search in the book

Press `?` to show this help

Press `Esc` to hide this help

# How to Enter an Address

You should enter an address as a hexadecimal number or a location name. When you enter the address in the hexadecimal format, you can omit the segment part of the address and the current segment will be used. Addresses beyond the program limits are invalid.

Also, you can enter a location name with a displacement:

            name+5

And finally you can specify a relative address:

            +10             0x10 bytes further
            -5              5 bytes backwards

If the entered string cannot be recognized as a hexadecimal number or location name, IDA will try to interpret it as an expression using the current script interpreter. The default interpreter is IDC.

Special addresses: $ - current location (depends on the current assembler) Examples:

`456` current segment, offset 0x456

`5E` current segment, offset 0x5E

`3000:34` segment 0x3000, offset 0x34

`ds:67` segment pointed by ds, offset 0x67

`0:4000000` linear address

`0x4000000` start a location with name ‘start’