## Keyboard shortcuts

Press `←` or `→` to navigate between chapters

Press `S` or `/` to search in the book

Press `?` to show this help

Press `Esc` to hide this help

# IDA supported processors

The list of supported processor/OS/file format combinations is so large that it is not easy to enumerate it. Please look at our gallery which contains disassembly samples across a wide number of processors.

## IDA Pro supported processors

IIDA Pro supports the processors listed below. The source code of some processor modules is available in our free SDK.

IDA Pro supported processors

- web assembly (WASM)
- AMD K6-2 3D-Now! extensions
- 32-bit ARM Architecture versions from v3 to v8 including Thumb, Thumb-2, DSP instructions and NEON Advanced SIMD instructions.
  - ARMv4 / ARMv4T: ARM7 cores (ARM7TDMI / ARM710T / ARM720T / ARM740T), ARM9 cores (ARM9TDMI / ARM920T / ARM922T / ARM940T)
  - ARMv5 / ARMv5TE / ARMv5TEJ: ARM9 cores (ARM946E-S/ ARM966E-S/ ARM968E-S/ ARM926EJ-S/ ARM996HS), ARM10E (ARM1020E / ARM1022E / ARM1026EJ-S)
  - ARMv6 / ARMv6T2 / ARMv6Z / ARMv6K: ARM11 cores (ARM1136J(F)-S / ARM1156T2(F)-S / ARM1176JZ(F)-S / ARM11 MPCore)
  - ARMv6-M: Cortex-M0 / Cortex-M0+ / Cortex-M1 (e.g. NXP LPC800/LPC1xxx, Freescale Kinetis L and M series, STM32 F0 series etc.)
  - ARMv7-M: Cortex-M3 (e.g. NXP LPC17xx/18xx/13xx, STM32 F1/F2/L1 series, TI Stellaris, Toshiba TX03 / TMPM3xx etc.)
  - ARMv7E-M: Cortex-M4 (e.g. NXP LPC43xx, STM32 F3/F4 series, TI Stellaris LM4F, Freescale Kinetis K series and W series, Atmel AT91SAM4 etc.)
  - ARMv7-R: Cortex-R4(F)/Cortex-R5/Cortex-R7 (e.g. TI TMS570LS etc.)
  - ARMv7-A: Cortex-A5 / Cortex-A7 / Cortex-A8 / Cortex-A9 / Cortex-A12 / Cortex-A15 (e.g. TI Sitara, TI OMAP series, Samsung S5PC100 and Exynos, Nvidia Tegra, Freescale i.MX, Allwinner A-Series and many others)
  - ARMv7 (custom): Apple A4/A5/A5X/A6/A6X (Swift microarchitecture, used in Apple’s iPhone/iPod/iPad/AppleTV), Qualcomm Snapdragon [Note: this list is incomplete; code for any ARM-compliant core can be disassembled]
- ARM64 Architecture (aka AArch64): *
  - ARMv8-A: Cortex-A50/Cortex-A53/Cortex-A57 etc.
  - ARMv8 (custom): Apple A7,A8 etc. (iPhone 5s and newer devices)
- ARC (Argonaut RISC Core), including ARCompact and ARCv2 (comes with source code)
- ATMEL AVR (comes with source code)
- DEC PDP-11(comes with source code)
- Fujitsu FR (comes with source code)
- Nintendo Entertainment System (NES) (6502)
- Nintendo Super Entertainment System (SNES) (65816, 65C816)
- Nintendo GameBoy (Z80, ARM7)
- Nintendo DS (ARM9, ARM11)
- Hitachi/Renesas H8/300, H8/300L, H8/300H, H8S/2000, H8S/2600, H8SX (comes with source code)H8/330, H8/322, H8/323, H8/325, H8/326-329, H8/336-338, H8/350, H8/3048F, H8/3202, H8/3212, H8/3214, H8/3216, H8/3217, H8/3256, H8/3257, H8/3292, H8/3294, H8/3296, H8/3297, H8/3315, H8/3318, H8/3334Y, H8/3336Y, H8/3337Y, H8/3337YF, H8/3394, H8/3396, H8/3397, H8/3534, H8/3434, H8/3434F, H8/3436, H8/3437, H8/3437F, H8/3522H8/3612, H8/3613, H8/3614, H8/3712, H8/3713, H8/3714, H8/3723, H8/3724, H8/3725, H8/3726, H8/3812, H8/3813, H8/3814, H8/3833-37, H8/3875, H8/3876, H8/3877, H8/3924, H8/3925, H8/3926, H8/3927, H8/3945-47H8/3002, H8/3040-3042, H8/3003, H8/3030-32, H8/3048, H8/3070, H8/3071, H8/3072H8S/2246, H8S/2245, H8S/2244, H8S/2243, H8S/2242, H8S/2241, H8S/2133, H8S/2144F, H8S/2357F, H8S/2143, H8S/2142F, H8S/2345F, H8S/2343, H8S/2341, H8S/2237, H8S/2235, H8S/2233, H8S/2227, H8S/2225, H8S/2223, H8S/2240, H8S/2242, H8S/2350, H8S/2352, H8S/2340, H8S/2355, H8S/2353, H8S/2351, H8S/2134F, H8S/2132FH8S/2655R, H8S/2653R, H8S/2655
- Hitachi H8/500 (comes with source code)
- Hitachi HD 6301, HD 6303, Hitachi HD 64180
- INTEL 8080
- INTEL 8085 (comes with source code)
- INTEL 80196 (comes with source code)
- INTEL 8051 (comes with source code)
- INTEL 860XR (comes with source code)
- INTEL 960 (comes with source code)
- INTEL 80×86 and 80×87 (Intel 8086/8088, 80186, 80286, 80386, 80486 and compatibles)
- INTEL Pentium/Celeron/Xeon, including SSE, SSE2, SSE3, SSE4, AVX, AVX2, AVX-512 and other extensions
- Java Virtual Machine (comes with source code)
- KR1878 (comes with source code)
- Microsoft .NET (Common Language Infrastructure bytecode)
- Mitsubishi MELPS740 or Renesas 740 (comes with source code)
- Hitachi/Renesas M16C family M16C/60, M16C/20, M16C/Tiny, R8C/Tiny, M16C/80, M32C/80, R32C/100
- MN102 (comes only with source code)
- MOS Technologies 6502, 65C02 (comes with source code)
- W65C816S aka 65C816 or 65816 (comes with source code)
- Motorola/Freescale 68K family: MC680xx, CPU32 (68330), MC6301
- Motorola 68xx series: MC6301, MC6303, MC6800, MC6801, MC6803, MC6805, MC6808, HCS08, MC6809, MC6811, \
- Motorola MC6812/MC68HC12/CPU12
- Freescale HCS12, HCS12X (including XGATE coprocessor)
- Motorola MC68HC16
- NSC CR16 (comes only with source code)
- NEC V850 series (including V850E1, V850E1F, V850ES, V850E2, V850E2M) (comes with source code)
- Renesas RH850 series (RH850G3K, RH850G3M, RH850G3KH, RH850G3MH) (comes with source code)
- EFI Byte Code (EBC) (comes with source code)
- SPU (Synergistic Processing Unit of the Cell BE) (comes with source code)
- MSP430, MSP430X (comes with source code)
- Microchip PIC 12XX, PIC 14XX, PIC 18XX, PIC 16XXX (comes with source code)
- Microchip 16-bit PIC series (PIC24, dsPIC: PIC24XX, PIC30XX, PIC33XX)
- Rockwell C39 (comes only with source code)
- Samsung SAM8 (comes with source code)
- SGS Thomson ST-7, and ST-20 (comes with source code)
- TLCS900 (comes only with source code)
- unSP from SunPlus
- Sony SPC700
- Philips XA series (51XA G3)(comes with source code)
- RISC-V
- Renesas RL78 series
- Intel xScale
- Z80, Zilog Z8, Zilog Z180, Zilog Z380 (comes with source code)
- IBM z/Architecture (S390, S390x)
- x64 architecture (aka Intel 64/IA-32e/EM64T/x86-64/AMD64)
- Analog Devices AD218x series (ADSP-2181, ADSP-2183, ADSP-2184(L/N), ADSP-2185(L/M/N), ADSP-2186(L/M/N), ADSP-2187(L/N), ADSP-2188M/N, ADSP-2189M/N)
- Dalvik (Android bytecode, DEX)
- DEC Alpha
- Motorola DSP563xx, DSP566xx, DSP561XX (comes with source code)
- TI TMS320C2X, TMS320C5X, TMS320C6X, TMS320C64X, TMS 320C54xx, TMS320C55xx, TMS320C3 (comes with source code)
- TI TMS320C27x/TMS320C28x
- Hewlett-Packard HP-PA aka PA-RISC (comes with source code)
- Hitachi/Renesas SuperH series. Unexhaustive list:
  - SH-1 core, for example SH7020,SH7021, SH7032,SH7034;
  - SH-2 core: SH7047, SH7049, SH7105, SH7107, SH7109 etc.;
  - SH-2E core: SH7055, SH7058 etc.;
  - SH-2A core: SH7201, SH7206, SH7211, SH7214
  - SH2A-FPU core: SH7450, SH7263 etc.;
  - SH3 core: SH7706, SH7709S;
  - SH4 core: SH7091(Sega Dreamcast), SH7750;
  - SH-4A core: SH7450, SH7451,SH7734, SH7785.
- Renesas RXv1, RXv2, RXv3 cores (RX100/RX200/RX600/RX700)
- IBM/Motorola PowerPC/POWER architecture, including Power ISA extensions:
  - Book E (Embedded Controller Instructions)
  - Freescale ISA extensions (isel etc.)
  - SPE (Signal Processing Engine) instructions
  - AltiVec (SIMD) instructions
  - Hypervisor and virtualization instructions
  - All instructions from the Power ISA 2.06 specification (Vector, Decimal Floating Point, Integer Multiply-Accumulate, VSX etc.)
  - Cell BE (Broadband Engine) instructions (used in PlayStation 3)
  - VLE (Variable Length Encoding) compressed instruction set
  - Xenon (Xbox 360) instructions, including VMX128 extension
  - Paired Single SIMD instructions (PowerPC 750CL/Gekko/Broadway/Espresso, used in Nintendo Wii and WiiU)
- Motorola/Freescale PowerPC-based cores and processors, including (but not limited to):
  - MPC5xx series: MPC533 / MPC535 / MPC555 / MPC556 / MPC561 / MPC562 / MPC563 / MPC564 / MPC566 Note: code compression features of MPC534/MPC564/MPC556/MPC566 (Burst Buffer Controller) are currently not supported
  - MPC8xx series (PowerQUICC): MPC821/MPC850/MPC860
  - MPC8xxx series (PowerQUICC II, PowerQUICC II Pro, PowerQUICC III): MPC82xx / MPC83xx / MPC85xx / MPC87xx
  - MPC5xxx series (Qorivva): MPC55xx, MPC56xx, MPC57xx
  - Power PC 4xx, 6xx, 74xx, e200 (including e200z0 with VLE), e500 (including e500v1, e500v2 and e500mc), e600, e700, e5500, e6500 cores
  - QorIQ series: P1, P2, P3, P4, P5 and T1, T2, T4 families
- Infineon Tricore: TC1xxx (AUDO, AUDO MAX), TC2xx, TC3xx, TC4x (AURIX, supported TriCore architecture up to v1.8)
- Intel IA-64 Architecture – Itanium.
- Motorola DSP 56K
- MIPS
  - MIPS Mark I (R2000)
  - MIPS Mark II (R3000)
  - MIPS Mark III: (R4000, R4200, R4300, R4400, and R4600)
  - MIPS Mark IV: R8000, R10000, R5900 (Playstation 2)
  - MIPS32, MIPS32r2, MIPS32r3 and MIPS64, MIPS64r2, MIPS64r3
  - Allegrex CPU (Playstation Portable – PSP), including VFPU instructions
  - Cavium Octeon and Octeon2 (cnMIPS) ISA extensions
  - MIPS16 (MIPS16e, MIPS16e2) Application Specific Extension
  - microMIPS Application Specific Extension
  - MIPS-MT, MIPS-3D, smartMIPS Application Specific Extensions
  - Toshiba TX19/TX19A Family Application Specific Extension (MIPS16e+ aka MIPS16e-TX)
- Mitsubishi M32R (comes with source code)
- Mitsubishi M7700 (comes with source code)
- Mitsubishi M7900 (comes with source code)
- Nec 78K0 and Nec 78K0S (comes with source code)
- STMicroelectronics ST9+, ST-10 (comes with source code)
- SPARCII, ULTRASPARC
- Siemens C166 (flow)
- Tensilica Xtensa
- Fujitsu F2MC-16L, Fujitsu F2MC-LC (comes with source code)

## IDA Home supported processors

IDA Home supported processors

IDA Home is available in 5 versions, each supporting one of the common processor families:

- x86/x64
- ARM/ARM64
- MIPS/MIPS64
- PowerPC/PPC64
- RISC-V/RV64

## Debugger Modules

In IDA Pro all debugger modules are available.

## Unsupported Processors

If your target processor is not included in the list above, you have two options:

1. Ask us to add support for the processor sometime in the future: we welcome your feedback about which processors should be added to IDA Pro.
2. Use our SDK and develop your own (free to all, but unsupported).