## Keyboard shortcuts

Press `←` or `→` to navigate between chapters

Press `S` or `/` to search in the book

Press `?` to show this help

Press `Esc` to hide this help

# TRICORE

Assembler code

    PFLASH:800000EC
    PFLASH:800000EC ; =============== S U B R O U T I N E =======================================
    PFLASH:800000EC
    PFLASH:800000EC
    PFLASH:800000EC                 .global asm_clear_endinit
    PFLASH:800000EC asm_clear_endinit:                      ; CODE XREF: _start+1C↑p
    PFLASH:800000EC                 ld32.w          d0, WDT_CON0 ; Watchdog Timer Control Register 0
    PFLASH:800000F0                 ld32.w          d1, WDT_CON1 ; Watchdog Timer Control Register 1
    PFLASH:800000F4                 movh            d2, #0
    PFLASH:800000F8                 addi            d2, d2, #-0xFF
    PFLASH:800000FC                 and16           d0, d2
    PFLASH:800000FE                 or32            d0, d0, #0xF0 ; 'ð'
    PFLASH:80000102                 and32           d4, d1, #0xC
    PFLASH:80000106                 or16            d0, d4
    PFLASH:80000108                 st32.w          WDT_CON0, d0 ; Watchdog Timer Control Register 0
    PFLASH:8000010C                 movh            d4, #0
    PFLASH:80000110                 addi            d4, d4, #-0x10
    PFLASH:80000114                 and16           d0, d4
    PFLASH:80000116                 or32            d0, d0, #2
    PFLASH:8000011A                 isync
    PFLASH:8000011E                 st32.w          WDT_CON0, d0 ; Watchdog Timer Control Register 0
    PFLASH:80000122                 ld32.w          d0, WDT_CON0 ; Watchdog Timer Control Register 0
    PFLASH:80000126                 nop16
    PFLASH:80000128                 ji16            a11
    PFLASH:80000128 ; End of function asm_clear_endinit
    PFLASH:80000128
    PFLASH:8000012A
    PFLASH:8000012A ; =============== S U B R O U T I N E =======================================
    PFLASH:8000012A
    PFLASH:8000012A
    PFLASH:8000012A                 .global _disable_wdt
    PFLASH:8000012A _disable_wdt:                           ; CODE XREF: _start:__no_board_init↑p
    PFLASH:8000012A                 movh            d2, #0
    PFLASH:8000012E                 addi            d2, d2, #-0xFD
    PFLASH:80000132                 movh            d5, #0